Jan 09, 2026

Package:
  EXL10e Released Engine Firmware v15.76

EXL10e Update Instructions:

1.  Unzip all files onto a Micro SD card.
2.  Plug the Micro SD card into a powered-up EXL10e.
3.  Press and hold SYSTEM until the Boot Installer Screen appears.
4.  Press Install Bootloader and Yes.
5.  When Operation Complete appears, press OK.
6.  Power-cycle the EXL10e and wait for it to boot up.
7.  Press SYSTEM, select View Status and press the Enter button.
8.  Scroll down to see the versions numbers, which should be:
    a.  Firmware Rev:  15.76
    b.  FPGA Rev:      0.7
    c.  InitRD Rev:    1.30
    d.  OS Ver:        2.6.35.86
9.  If any of the version numbers don't match, repeat steps 3 through 8.
