18-Dec-2012

This .zip file or folder contains all files necessary to field-update a Horner
XL4e to the latest release, which includes the following:

    Firmware:              12.94
    FPGA image:            0.3
    Boot Loader (InitRD):  1.01
    Kernel:                2.6.35.26

To update a Horner XL4e:

    1.  Using an available PC USB slot or Micro SD card reader, copy the files
    	from this folder into the root directory of a FAT-formatted USB Flash
    	Drive or a (2 GB or smaller) Micro SD Flash Card.

    2.  IMPORTANT:  First, eject the USB or Micro SD media from the PC, so it
    	can be safely removed.  Then remove it from the PC.

    3.  Plug the media into a powered-up XL4e.

    4.  On the XL4e, hold the SYSTEM key down for 5 seconds to display the
        Boot Installer Screen.

    5.  Touch the Install Bootloader button and then touch Yes.
    
    6.	When the Operation Completed message appears (after about 13 seconds),
    	touch OK.

    7.  Hold down SYSTEM and F2 for two seconds to reboot and run the new
    	kernel and firmware.
