June 24, 2025

Package:
  XL4e-CsCAN Released Engine Firmware v15.74

XL4e-CsCAN Update Instructions:

1.  Unzip all files onto a Micro SD card.
2.  Plug the Micro SD card into a powered-up XL4e.
3.  Press and hold SYSTEM until the Boot Installer Screen appears.
4.  Press Install Bootloader and Yes.
5.  When Operation Complete appears, press OK.
6.  Power-cycle the XL4e and wait for it to boot up.
7.  Press SYSTEM, select View Status and press the Enter button.
8.  Scroll down to see the versions numbers, which should be:
    a.  Firmware Rev:  15.74
    b.  FPGA Rev:      0.7
    c.  InitRD Rev:    1.30
    d.  OS Ver:        2.6.35.86
9.  If any of the version numbers don't match, repeat steps 3 through 8.
